|  |  |
| --- | --- |
| Address | Value |
| $sp0,$fp1-> |  |
|  | $fp0(initial value of fp) |
|  | $ra0(return address of WARP procedure) |
| $sp1,$fp2-> |  |
|  | $fp1 |
|  | $ra |
|  | $a0 = 3 |
| $sp2,$fp3-> |  |
|  | $fp2 |
|  | $ra |
|  | $a0 = 2 |
| $sp3,$fp4-> |  |
|  | $fp3 |
|  | $ra |
|  | $a0 = 1 |